TransSlantRollOut AviSynth Plugin

# TransSlantRollOut

Left (first) clip rolls out along the diagonals as a carpet over the Right (second) clip revealing it. Roll diameter, style of shading and the direction (four) of rolling are the parameters that can be specified. RGB32, RGB24 YV12 and YUY2 colorspaces only are supported.

Details of parameters
Description | Name | Type | Limits | Default
Left clip |  | clip |  | none
Right clip |  | clip |  | none
Overlapping frames or seconds time | overlap | integer | not more than clip length , >2 frames. If -ve taken as time in seconds | none
direction of Roll in | dir | string | "se", "ne", "sw', "nw" | "se"
Maximum diameter of Roll in pixels | rolldia | integer | minimum 8 and not more than 1/4th of smaller of frame dimensions | 80
shading of roll. . zero means no shading. _ve value for edges shaded more while + ve value shades center more. | shade | integer | -255 to 255 | 127

#Usage examples:-
TransSlantRollOut(Left, Right,100,"se",120,-60)
TransSlantRollOut(Left, Right,-4, rolldia=120)
TransSlantRollOut(Left, Right,-4)
Images during Transition with dir='sw' option:

Back to Synopsys. |  |
| Back to my page |
|  | back to Avisynth