TransRipple AviSynth Plugin

# TransRipple

A gradually increasing water ripple that covers fully the Left Clip by 1/3 overlap length is created. Thereafter the Right Clip emerges in the center as a growing Ripple fully covering frame by 2/3 length. This ripple then subsides (withdraws) over the Right Clip thus revealing it. The wave length lambda and wave amplitude may be specified. RGB32, RGB24 YV12 and YUY2 colorspaces only are supported.

Details of parameters
Description | Name | Type | Limits | Default
Left clip |  | clip |  | none
Right clip |  | clip |  | none
Overlapping frames or seconds time | overlap | integer | not more than clip length , >2 frames. If -ve taken as time in seconds | none
Wave length | lambda | integer | more than 15 and less than 1/8 of frame diagonal | 40
Wave amplitude | amp | integer | between 2 and 12 | 8

#Usage examples:-

    TransRipple(Left,Right,-3,80,4)
    TransRipple(Left,Right,-3)
    TransRipple(Left,Right, -3,amp=4)
    TransRipple(Left,Right,-3,lambda=60)

Images during transition :

Back to Synopsys. |  |
| Back to my page |
|  | back to Avisynth